Ordering Instructions for Low-Voltage Switchgear

If you choose our products, please provide the following data in order to provide you with better
	Project
	Technical Requirements/Options

	Product Type
	□ MNS □ GCS □ GCK □ GGD □  Other          

	Rated Voltage
	         V (e.g. AC400V)

	Main Busbar
	         A (e.g. 4000A, 6300A) / □ Copper □ Aluminum

	Short-time Withstand Current
	         kA/1s (e.g. 50kA)

	Protection Degree
	□ IP30 □ IP40 □ IP54 (Outdoor)

	Feeder Circuits
	Incomer:          circuit / Outgoing:           circuit

	Enclosure
	□ Fixed □ Withdrawable

	Smart Monitoring
	□ Temp. Sensor □ RS485/Modbus

	Environment
	Humidity:          % / Ambient Temp:          ℃

	Color
	□ RAL7035 (Standard gray) □ 定制          

	Special Requirements
	                                                              

	Order Quantity
	              (pcs)

	Delivery Lead Time
	              (YYYY/MM/DD)

	Deliver y met hod
	                                         

	Modes of transport
	                                         

	Place of delivery
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